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	Response actions (as appropriate)

	When a volcano threatens


	 Listen to your radio or TV for advice and information 

	
	 Contact your local Civil Defence Group for advice.

	
	 Check that staff know what to do. 

	Large eruption

	 Evacuation: If the site is in the path of potential lava flows, pyroclastic flows, surges or lahars be prepared to evacuate when asked to by controlling authorities (i.e. police, civil defence etc).   

	Ash Fall


	 Ensure that staff and visitors stay indoors. Have dust masks available. 

	
	 Close windows and doors. In heavy ash falls, windows and doors may need additional sealing to avoid ash entering buildings.  

	
	 Turn off air-conditioning units and any other equipment that draws in or blows air. 

	
	 Protective clothing (especially if working in the ash fall) should be worn by anyone who has to work outside in an emergency and goggles used to protect the eyes. 

	
	 Monitor the amount of ash on roofs.  Roofs may collapse under the weight of ash causing injury to the occupants.  Evacuate buildings which show signs of roof sagging. 

	
	 Disconnect roof-fed water supply only when ash fall is occurring or during the clean up to stop ash entering the storage tanks. 

	
	 If possible have l outdoor equipment, cars etc parked under-cover or cover them. 

	Cleaning up after an ash fall
	The local council and CDEM group will provide advice on cleaning up and disposing of ash. 



